

Câu 2:


Ping from PC0 to PC2



Ping from PC2 to PC0





Ping from PC1 to PC3



Ping from PC3 to PC1


2.





3.

Line is configured by static route in R0:



Text

Description automatically generated

* The number in red square is the administrative distance (“1” means static route), the number in the blue square is the metric of static route (“0” is the cost of a route).